# -*- sh -*-
# Copyright (c) 2004-2005 The Trustees of Indiana University and Indiana
#                         University Research and Technology
#                         Corporation.  All rights reserved.
# Copyright (c) 2004-2005 The University of Tennessee and The University
#                         of Tennessee Research Foundation.  All rights
#                         reserved.
# Copyright (c) 2004-2005 High Performance Computing Center Stuttgart, 
#                         University of Stuttgart.  All rights reserved.
# Copyright (c) 2004-2005 The Regents of the University of California.
#                         All rights reserved.
# $COPYRIGHT$
# 
# Additional copyrights may follow
# 
# $HEADER$
#

#
# Database for mapping architecture and assembly format to prebuilt
# assembly files.  For explination of the assembly operations, see
# the inline assembly header files in src/include/sys/<arch>.
#
# FORMAT:
# ARCHITECTURE	ASSEMBLY FORMAT			BASE FILENAME
#
# Assembly Format field:
#   config_file-text-global-label_suffix-gsym-lsym-type-size-align_log-ppc_r_reg-64_bit-gnu_stack

######################################################################
#
# Alpha
#
######################################################################

ALPHA	default-.text-.globl-:--$-@-1-1-1-1-1	alpha-linux


######################################################################
#
# AMD Opteron / Intel EM64T
#
######################################################################

AMD64	default-.text-.globl-:--.L-@-1-0-1-1-1	amd64-linux
AMD64	default-.text-.globl-:--.L-@-1-0-1-1-0	amd64-linux-nongas


######################################################################
#
# ARM (ARMv7 and later)
#
######################################################################

ARM    default-.text-.globl-:--.L-#-1-1-1-1-1  arm-linux


######################################################################
#
# Intel Pentium Class
#
######################################################################

IA32	default-.text-.globl-:--.L-@-1-0-1-1-1	ia32-linux
IA32	default-.text-.globl-:--.L-@-1-0-1-1-0	ia32-linux-nongas
IA32	default-.text-.globl-:-_-L--0-1-1-1-0	ia32-osx
IA32	default-.text-.globl-:-_-L--0-0-1-1-1	ia32-cygwin
IA32	default-.text-.globl-:-_-L--0-0-1-1-0	ia32-cygwin-nongas


######################################################################
#
# IA64 (Intel Itanium)
#
######################################################################

IA64	default-.text-.globl-:--.L-@-1-0-1-1-1	ia64-linux
IA64	default-.text-.globl-:--.L-@-1-0-1-1-0	ia64-linux-nongas


######################################################################
#
# PowerPC / POWER 
#
######################################################################

# standard ppc instruction set (AIX calls it ppc).  This is not the
# true intersection of all the POWER / PowerPC machines, but works
# on PowerPCs since the 601 and on at least POWER 3 and above.
POWERPC32	default-.text-.globl-:-_-L--0-1-1-0-0	powerpc32-osx
POWERPC32	default-.text-.globl-:--.L-@-1-1-0-0-1	powerpc32-linux
POWERPC32	default-.text-.globl-:--.L-@-1-1-0-0-0	powerpc32-linux-nongas
POWERPC32	aix-.csect .text[PR]-.globl-:-.-L--0-1-0-0-0	powerpc32-aix

# The ppc code above, plus support for the 64 bit operations.  This
# mode is really only available on OS X when using the OS X 10.3
# compiler chain with the -mcpu=970 option.
POWERPC32	default-.text-.globl-:-_-L--0-1-1-1-0	powerpc32-64-osx

# PowerPC / POWER 64bit machines.  sizeof(void*) == 8.
POWERPC64	default-.text-.globl-:-_-L--0-1-1-1-0	powerpc64-osx
POWERPC64	default-.text-.globl-:-.-.L-@-1-1-0-1-1	powerpc64-linux
POWERPC64	default-.text-.globl-:-.-.L-@-1-1-0-1-0	powerpc64-linux-nongas
POWERPC64	aix-.csect .text[PR]-.globl-:-.-L--0-1-0-1-0	powerpc64-aix


######################################################################
#
# SPARC / UltraSPARC (Scalalable Processor ARChitecture)
#
######################################################################

# default compile mode on Solaris.  Evil.  equiv to about Sparc v8
SPARC	default-.text-.globl-:--.L-#-1-0-1-0-0	sparc-solaris

# Usually compiled with -xarch=v8plus.  Basically Sparc V9, but with
# sizeof(void*) == 4 instead of 8.  Different from V9_64 because still
# uses 2 registers to pass in a 64bit integer
SPARCV9_32	default-.text-.globl-:--.L-#-1-0-1-1-0	sparcv9-32-solaris

# The Sparc v9 (aka Ultra Sparc).  Sizeof(void*) == 8.
SPARCV9_64	default-.text-.globl-:--.L-#-1-0-1-1-0	sparcv9-64-solaris


######################################################################
#
# MIPS III (Microprocessor without Interlocked Pipeline Stages)
#          R4000 and above
#
######################################################################

# So MIPS, in it's infinite wisdom (thank you!) decided that when
# compiling in 32bit mode and passing in a 64bit integer, it is done
# in one register (instead of SPARC and POWER, who use two).  Which
# means that we can use the same code either way.  Woo hoo!

MIPS	default-.text-.globl-:--L--1-1-1-1-0	mips-irix
MIPS	default-.text-.globl-:--L--1-1-1-1-0	mips64el
MIPS	default-.text-.globl-:--L-@-1-1-1-1-1	mips64-linux

# However, this doesn't hold true for 32-bit MIPS as used on Linux.
MIPS	default-.text-.globl-:--L-@-1-1-1-0-1	mips-linux
