# -*- text -*-
#
# Copyright (c) 2008-2009 Cisco Systems, Inc.  All rights reserved.
# $COPYRIGHT$
# 
# Additional copyrights may follow
# 
# $HEADER$
#
# This is the US/English help file for Open MPI's OpenFabrics IB CPC
# support.
#
[no cpcs for port]
No OpenFabrics connection schemes reported that they were able to be
used on a specific port.  As such, the openib BTL (OpenFabrics
support) will be disabled for this port.

  Local host:           %s
  Local device:         %s
  Local port:           %d
  CPCs attempted:       %s
#
[cpc name not found]
An invalid CPC name was specified via the btl_openib_cpc_%s MCA 
parameter.

  Local host:                   %s
  btl_openib_cpc_%s value: %s
  Invalid name:                 %s
  All possible valid names:     %s
#
[inline truncated]
WARNING: The btl_openib_max_inline_data MCA parameter was used to
specify how much inline data should be used, but a device reduced this
value.  This is not an error; it simply means that your run will use
a smaller inline data value than was requested.

  Local host:           %s
  Local device:         %s
  Local port:           %d
  Requested value:      %d
  Value used by device: %d
